Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### STP Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure the Pseudo Root ID

- Specify the interface for the BPDU transmit status and configure the pseudo root ID of the L2GP.

      SEFOS# configure terminal
      SEFOS(config)# interface extreme-ethernet 0/1
      SEFOS(config)# spanning-tree pseudoRootId priority 4096 mac-address 00:01:02:03:04:01

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |