Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### STP Administration Guide

Search Scope:

- This Document
- Entire Library

### Default STP Settings

Feature | Default Setting
--- | ---
Spanning tree mode | MSTP
Spanning tree status | Enabled
Spanning tree timers | Hello time: 2 secondsForward-delay time: 15 seconds.Maximum-aging time: 20 seconds.
Switch priority | 32768
Spanning tree port priority (configurable on a per-interface basis) | 128
Spanning tree port cost (configurable on a per-interface basis) | 200000 (For RSTP, the default value is 65535)

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |