Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### IPv6 Administration Guide

Search Scope:

- This Document
- Entire Library

## Add IPv6 Addresses to an Interface

1. Enter Interface Configuration mode for `VLAN 1`, and enable IPv6.

       SEFOS# configure terminal
       SEFOS(config)# interface vlan 1
       SEFOS(config-if)# ipv6 enable

2. Assign IPv6 address for the interface.

       SEFOS(config-if)# ipv6 address fec0::1111:0:1/96

   The default prefix type is set as unicast. You can configure the prefix type as anycast, eui64, or link-local address by defining the prefix type in the command.

3. Configure the IPv6 link-local address for the interface.

       SEFOS(config-if)# ipv6 address fe80::203:2ff:fe03:501 link-local
       SEFOS(config-if)# end

4. Review the IPv6 information for the `VLAN 1` interface.

       SEFOS# show ipv6 interface vlan 1

       vlan1 is up, line protocol is up
           IPv6 is Enabled
           Link local address:
               fe80::203:2ff:fe03:501
           Global unicast address(es):
               fec0::1111:0:1/96
       ...

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |