Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### PIMv6 Administration Guide

Search Scope:

- This Document
- Entire Library

## Enable PIMv6

By default, PIMv6 is disabled in the system. Enable PIMv6 in all of the routers in a network that need to support PIMv6 (for example, router A and router B in the example topology).

1. Enable PIMv6 in the router.

       SEFOS# configure terminal
       SEFOS(config)# set ip pim enable
       SEFOS(config)# set ipv6 pim enable
       SEFOS(config)# end

2. Review the configuration information.

       SEFOS# show ipv6 pim component

       PIM Component Information
       ---------------------------
       Component-Id: 1
         PIM Mode: sparse,   PIM Version: 2
         Elected BSR: ::
         Candidate RP Holdtime: 0

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |