Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### PIM Administration Guide

Search Scope:

- This Document
- Entire Library

## Display RP Details

After configuring a static RP, you can view the group prefix, RP address, and hold and expiration times for the interface.

1. Enable static RP.

       SEFOS# configure terminal
       SEFOS(config)# set ip pim static-rp enable
       SEFOS(config)# interface vlan 5
       SEFOS(config-if)# ip pim componentId 1

2. Specify how often (in seconds) the switch sends PIM messages to the interface.

       SEFOS(config-if)# ip pim query-interval 60

3. Configure the BSR.

       SEFOS(config-if)# ip pim bsr-candidate 30
       SEFOS(config-if)# exit

4. Configure the RP candidate.

       SEFOS(config)# ip pim component 1
       SEFOS(pim-comp)# rp-candidate holdtime 30
       SEFOS(pim-comp)# rp-candidate rp-address 224.1.0.0 255.255.0.0 10.1.0.1
       SEFOS(pim-comp)# end

5. Configure PIM component 1.

       SEFOS(config)# ip pim component 1

6. Configure the RP-static RP-address `10.1.0.1` for the group `224.1.0.0/16` in PIM component 1.

       SEFOS(pim-comp)# rp-static rp-address 224.1.0.0  255.255.0.0  10.1.0.1
       SEFOS(pim-comp)# end

7. View the RP details for the interface (in this example, PIM component 1).

       SEFOS# show ip pim rp-set

       PIM Group-to-RP mappings
       ------------------------
       Group Address : 224.1.0.0 Group Mask : 255.255.0.0
          RP: 10.1.0.1
         Component-Id : 1
           Hold Time : 30, Expiry Time : 00:00:19

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |