Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### SLB Administration Guide

Search Scope:

- This Document
- Entire Library

#### SLB-L2 Failover Example

SLB-L2 monitors the link interface between the server and the switch. When the link fails, a failover event takes place. SLB-L2 provides several failover options. Refer to the`slb l2 failover-method` command in the Sun Ethernet Fabric Operating System CLI Base Reference Manual for more information.

The following example illustrates a failover event. The LBG in this example has four active nodes.

    SEFOS# show slb l2

    L2 SLB Group #1
    Failover Method: Failover to All ports

    Port Members:
    Port   State     Comments
    ====   =====     =================
     15    ACTIVE
     16    ACTIVE
     17    ACTIVE
     18    ACTIVE

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |