Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### VLAN Administration Guide

Search Scope:

- This Document
- Entire Library

### Default Settings

The following table lists the default settings for the switch.

Feature | Default Setting
--- | ---
VLAN module status | Enable
Default VLAN ID (configured in the switch) | 1
System and port level GVRP and GMRP module status | Enabled
MAC address table aging time | 300 seconds
Acceptable frame types | All (accepts untagged frames or priority-tagged frames or tagged frames received on the port)
Ingress filtering | Disabled
Switch port priority | 0
Switch port mode | Hybrid
GARP timers | Join: 20 secondsLeave: 60 secondsLeave all: 1000 seconds
Max traffic classes | Maximum number of traffic classes supported on a port is 8.
Tunneling | Disabled

The following illustration shows a typical topology for a VLAN configuration in which two switches are connected to each other. Host A represents the terminal access to the VLAN.

Copyright © 2010, 2011, Oracle and/or its affiliates. All rights reserved. Legal Notices |