Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### PVRST+ Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure the Spanning Tree Link Type

If a port is configured as a point-to-point link and its port role is designated, then PVRST+ negotiates a rapid transition to the forwarding state with the other port by using a proposal-handshake agreement mechanism to ensure that the topology is loop free. By default, if the interface is full-duplex, then it is considered to have a point-to-point connection. The default setting of link type can be overridden to enable rapid transition to the forwarding state.

1. In switch C, specify the interface for which the link type is to be configured.

       TOR-2 SEFOS# configure terminal
       TOR-2 SEFOS(config)# interface extreme-ethernet 0/1

   Valid interfaces include physical interfaces and port-channel logical interfaces (`port-channel` port_channel_number).

2. Configure the link type of the interface as point-to-point.

       TOR-2 SEFOS(config-if)# spanning-tree link-type point-to-point
       TOR-2 SEFOS(config-if)# end

3. Review the spanning tree properties.

       TOR-2 SEFOS# show spanning-tree vlan 10

       -------------------------------------------------------------------
       Spanning-tree for VLAN 10
       Root Id         Priority   32778
                       Address    00:14:4f:6c:56:6f
                       Cost       2000
                       Port       Ex0/1
                       Hello Time 2 Sec, Max Age 20 Sec, Forward Delay 15 Sec
       Spanning Tree Enabled Protocol PVRST
       Bridge Id       Priority 32778
                       Address 00:14:4f:6c:6e:0d
                       Hello Time 2 sec, Max Age 20 sec, Forward Delay 15 sec
       Name     Role         State        Cost     Prio   Type
       ----     ----         -----        ----     ----   ------
       Ex0/1    Root         Forwarding   2000     128    P2P
       Ex0/57   Alternate    Discarding   2000     128    P2P

       TOR-2 SEFOS#

4. Reset the default link type for the interface.

       TOR-2 SEFOS# configure terminal
       TOR-2 SEFOS(config)# interface extreme-ethernet 0/1
       TOR-2 SEFOS(config-if)# no spanning-tree link-type
       TOR-2 SEFOS(config-if)# end
       TOR-2 SEFOS#

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |