Skip Navigation Links
Exit Print View
| Sun Network 10GbE Switch 72p ### User’s Guide

Search Scope:

- This Document
- Entire Library

## Verify the DHCP-Assigned IP Address and Host Name

Note - By default, the switch is configured to use DHCP to automatically obtain an IP address.

Note - You must configure an externally accessible IP address on the switch to use SNMP. Refer to the following documentation for more information on using SNMP with the switch: Sun Integrated Lights Out Manager (ILOM) 3.0 Management Protocols Reference Guide and Sun Network 10GbE Switch 72p Software Configuration Guide.

1. Log into the DHCP server and obtain the IP address assigned to the switch.
2. ...?
3. Consider your next steps.

   - Log into Oracle ILOM web.

     See Log Into Oracle ILOM Web (NET MGT).

   - Log into Oracle ILOM CLI.

     See Log Into Oracle ILOM CLI (NET MGT).

##### Related Information

- Oracle ILOM Overview

- Configure Network Management From CLI (SER MGT)

- Log Into Oracle ILOM Web (NET MGT)

- Log Into Oracle ILOM CLI (NET MGT)

- Log Into Oracle ILOM CLI (SER MGT)

- Configure Network Management From Web

- Configure Network Management From CLI (NET MGT)

- Log Out of ILOM

Copyright © 2011, 2012 , Oracle and/or its affiliates. All rights reserved. Legal Notices |