Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### PIMv6 Administration Guide

Search Scope:

- This Document
- Entire Library

## Associate the PIMv6 Component to an Interface

The `ipv6 pim componentId` command adds an interface to the PIMv6 component and enables PIMv6 on the interface. You must associate a PIMv6 component with the interface to turn the interface into a supported PIMv6 module. In addition, you must create a component before you associate that component with an interface, except for the default component 1. See Configuring the PIMv6 Component for instructions on how to create a component.

1. Enable PIMv6.

       SEFOS# configure terminal
       SEFOS(config)# set ipv6 pim enable

2. Enter the configuration mode for `VLAN 1`, and associate the VLAN interface with the PIMv6 component ID (2 in this case).

       SEFOS(config)# interface vlan 1
       SEFOS(config-if)# ipv6 pim componentId 2
       SEFOS(config-if)# end

3. Review the interface status.

       SEFOS# show ipv6 pim interface detail

       ...
           PIM Lan-Prune-Delay : Disabled
           PIM Component Id : 2
       ...

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |