C H A P T E R 5

PIMv6

PIMv6 is a portable software implementation of the PIM (sparse mode) specification for IPv6 networks. PIMv6 provides support for inter-domain routing between domains using PIMv6-SM. It also avoids the performance problems of earlier multicast routing protocols. This software provides multicast routing and forwarding capabilities to a router that runs the IPv6 protocol along with MLD. PIMv6 routes multicast data packets independent of any unicast routing protocol.

##

5.1 PIMv6 Commands

The list of CLI commands for the configuration of PIMv6 is as follows:

- set ip pim

- set ipv6 pim

- set ip pim threshold

- set ip pim spt-switchperiod

- set ip pim rp-threshold

- set ip pim rp-switchperiod

- set ip pim regstop-ratelimit-period

- set ip pim pmbr

- set ip pim static-rp

- ip pim component

- ipv6 pim rp-candidate rp-address

- ipv6 pim rp-static rp-address

- ipv6 pim query-interval

- ipv6 pim message-interval

- ipv6 pim bsr-candidate

- ipv6 pim componentId

- ipv6 pim dr-priority

- ipv6 pim override-interval

- ipv6 pim lan-delay

- set ipv6 pim lan-prune-delay

- no ipv6 pim interface

- debug ipv6 pim

- show ipv6 pim interface

- show ipv6 pim neighbor

- show ipv6 pim rp-candidate

- show ipv6 pim rp-set

- show ipv6 pim bsr

- show ipv6 pim rp-static

- show ipv6 pim component

- show ipv6 pim thresholds

- show ipv6 pim mroute

### 5.1.1 `set ip pim`

Enables or disables PIM globally.

Note - In addition to the set ipv6 pim `enable` command, the set ip pim `enable` command must be executed to enable PIMv6.

    set ip pim {enable | disable}

Syntax Description | enable - Enables PIM. disable - Disables PIM.
Mode | Global Configuration
Defaults | Disabled.
Example | SEFOS(config)# set ip pim enable
Notes | PIM mode will be set as sparse, when PIM is enabled globally. IGMP proxy service must be disabled in the system, before enabling the PIM globally.

### 5.1.2 `set ipv6 pim`

Enables or disables PIMv6 globally.

    set ipv6 pim {enable | disable}

Syntax Description | enable - Enables PIMv6. disable - Disables PIMv6.
Mode | Global Configuration
Defaults | Disabled.
Example | SEFOS (config)# set ipv6 pim enable
Notes | When PIMv6 is globally enabled, the mode will be sparse.

#### Related Commands

- no ipv6 pim interface - Displays the PIMv6 interfaces of the router

### 5.1.3 `set ip pim threshold`

Configures the SPT group or source threshold, when exceeded, switching to shortest path tree is initiated.

    set ip pim threshold {spt-grp | spt-src} number-of-packets_0-2147483647

Syntax Description | spt-grp - The threshold of data rate for any group. When exceeded, source specific counters are initiated for that particular group. It is based on number of bits per second. spt-src - The switching to shortest path tree is initiated when the threshold of data rate for any source is exceeded. It is based on number of bits per second. number-of-packets_0-2147483647 - Number of packets.
Mode | Global Configuration
Defaults | 0
Example | SEFOS (config)# set ip pim threshold spt-grp 50

#### Related Commands

- show ipv6 pim thresholds - Displays threshold configured for SPT, RP thresholds, rate limit values for both SM and DM

### 5.1.4 `set ip pim spt-switchperiod`

Configures the period (in seconds) over which the data rate is to be monitored for switching to shortest path tree.

    set ip pim spt-switchperiod seconds_0-2147483647

Mode | Global Configuration
Defaults | 0
Example | SEFOS (config)# set ip pim spt-switchperiod 60
Notes | The same period is used for monitoring the data rate for both source and group. To switch to SPT, this period must be configured. The SPT is used for multicast transmission of packets with the shortest path from sender to recipients.

#### Related Commands

- show ipv6 pim thresholds - Displays threshold configured for SPT, RP thresholds, rate limit values for both SM and DM

### 5.1.5 `set ip pim rp-threshold`

Sets the threshold at which RP initiates switching to source specific shortest path tree.

    set ip pim rp-threshold number-of-reg-pkts_0-2147483647

Mode | Global Configuration
Example | SEFOS (config)# set ip pim rp-threshold 200

#### Related Commands

- show ipv6 pim thresholds - Displays threshold configured for SPT, RP thresholds, rate limit values for both SM and DM

### 5.1.6 `set ip pim rp-switchperiod`

Sets the period (in seconds) over which RP monitors register packets for switching to the source specific shortest path tree.

    set ip pim rp-switchperiod seconds_0-2147483647

Mode | Global Configuration
Defaults | 0
Example | SEFOS (config)# set ip pim rp-switchperiod 100
Notes | To switch to SPT, this period must be configured RP-tree is a pattern that multicast packets are sent to a PIM-SM router by unicast and then forwarded to actual recipients from RP

#### Related Commands

- show ipv6 pim thresholds - Displays threshold configured for SPT, RP thresholds, rate limit values for both SM and DM

### 5.1.7 `set ip pim regstop-ratelimit-period`

Sets the period over which RP monitors the number of register packets after sending the register stop message.

    set ip pim regstop-ratelimit-period seconds_0-2147483647

Mode | Global Configuration
Defaults | 5
Example | SEFOS (config)# set ip pim regstop-ratelimit-period 100
Notes | The register stop message is used to avoid encapsulation of multicast data packets from the first hop router to the RP.

#### Related Commands

- show ipv6 pim thresholds - Displays threshold configured for SPT, RP thresholds, rate limit values for both SM and DM

### 5.1.8 `set ip pim pmbr`

Enables or disables the PMBR (PIM multicast border router) status.

    set ip pim pmbr {enable | disable}

Syntax Description | enable - Enables the PMBR status. disable - Disables the PMBR status.
Mode | Global Configuration
Defaults | Disabled.
Example | SEFOS (config)# set ip pim pmbr enable
Notes | A PMBR integrates two different PIM domains (either PIM-SM or PIM-DM). A PMBR connects a PIM domain to other multicast routing domain(s).

#### Related Commands

- show ipv6 pim thresholds - Displays threshold configured for SPT, RP thresholds, rate limit values for both SM and DM

### 5.1.9 `set ip pim static-rp`

Enables or disables the static RP configuration status. This command specifies whether to use the configured static RP.

    set ip pim static-rp {enable | disable}

Syntax Description | enable - Enables the static RP configuration status. disable - Disables the static RP configuration status.
Mode | Global Configuration
Defaults | Disabled.
Example | SEFOS (config)# set ip pim static-rp enable

#### Related Commands

- show ipv6 pim rp-set - Displays the RP-set information

- show ipv6 pim rp-static - Displays the RP-static information

### 5.1.10 `ip pim component`

Configures the PIMv6 component in the router. The `no` form of the command destroys the PIMv6 component.

    ip pim component component-id_1-255

    no ip pim component component-id_1-255

Mode | Global Configuration
Example | SEFOS(config)# ip pim component 1
Notes | PIMv6 component 1 cannot be deleted, as it is the default component. The PIMv6 component corresponds to each instance of a PIMv6 domain and classifies it as sparse or dense mode. Currently, only sparse mode is supported.

#### Related Commands

- show ipv6 pim component - Displays the component information

### 5.1.11 `ipv6 pim rp-candidate rp-address`

Sets the address of the interface, which will be advertised as a candidate-RP. The `no` form of the command disables the address of the interface, which will be advertised as a candidate-RP.

    ipv6 pim rp-candidate rp-address group-address group-mask rp-address

    no ipv6 pim rp-candidate rp-address group-address group-mask rp-address

Syntax Description | group-address - IPv6 multicast group address. group-mask - IPv6 multicast group address mask that gives the group prefix for which the entry contains information about RP. rp-address - IPv6 address of the rendezvous point.
Mode | PIM Component
Example | SEFOS(pim-comp)# ipv6 pim rp-candidate rp-address ff02::e001:0000 112 3333::1111
Notes | A candidate-RP is a router configured to send periodic candidate-RP-advertisement messages to the BSR, and processes join/prune or register messages for the advertised group prefix, when it is elected as a RP.

#### Related Commands

- show ipv6 pim rp-set - Displays the PIMv6 RP-set information

- show ipv6 pim rp-candidate - Displays the PIMv6 RP-candidate information

### 5.1.12 `ipv6 pim rp-static rp-address`

Sets the address of the IPv6 interface, which will be advertised as a Static-RP. The `no` form of the command disables the address of the IPv6 interface, which will be advertised as a Static-RP.

    ipv6 pim rp-static rp-address group-address group-mask rp-address

    no ipv6 pim rp-static rp-address group-address group-mask rp-address

Syntax Description | group-address - IPv6 multicast group address. group-mask - IPv6 multicast group address mask that gives the group prefix for which the entry contains information about RP. rp-address - IPv6 address of the rendezvous point.
Mode | PIM Component
Example | SEFOS(pim-comp)# ipv6 pim rp-static rp-address ff02::e001:0000 112 3333::1111
Notes | The static configuration allows additional structuring of the multicast traffic by directing the multicast join or prune messages to statically configured RPs.

#### Related Commands

- show ipv6 pim rp-static - Displays the RP-static information

### 5.1.13 `ipv6 pim query-interval`

Sets the frequency at which PIMv6 hello messages are transmitted on the interface. The `no` form of the command sets the default hello timer interval for the interface.

    ipv6 pim query-interval seconds_0-65535

    no ipv6 pim query-interval

Mode | Interface Configuration
Defaults | 30
Example | SEFOS (config-if)# ipv6 pim query-interval 60
Notes | The query message informs the presence of a PIMv6 router on the interface to the neighboring PIMv6 routers.

#### Related Commands

- show ipv6 pim interface - Displays the PIMv6 interfaces of the router

### 5.1.14 `ipv6 pim message-interval`

Sets the frequency at which the PIMv6 join or prune messages are transmitted on the PIMv6 interface. The `no` form of the command sets the default value for the PIMv6 join/prune messages.

    ipv6 pim message-interval seconds_0-65535

    no ipv6 pim message-interval

Mode | Interface Configuration
Defaults | 60
Example | SEFOS (config-if)# ipv6 pim message-interval 120
Notes | The join/prune message interval used on all the PIMv6 routers in the PIMv6 domain must be the same. If all the routers do not use the same timer interval, the performance of PIMv6 sparse can be adversely affected.

#### Related Commands

- show ipv6 pim interface - Displays the PIMv6 interfaces of the router.

### 5.1.15 `ipv6 pim bsr-candidate`

Sets the preference value for the local PIMv6 interface as a candidate bootstrap router. The `no` form of the command sets the default preference value for the local PIMv6 interface as a candidate bootstrap router.

    ipv6 pim bsr-candidate 0-255

    no ipv6 pim bsr-candidate

Mode | Interface Configuration
Defaults | 0
Example | SEFOS (config-if)# ipv6 pim bsr-candidate 1
Notes | A BSR is a dynamically elected router within the PIMv6 domain.

#### Related Commands

- show ipv6 pim bsr - Displays the PIMv6 BSR information

### 5.1.16 `ipv6 pim componentId`

Adds the interface to the component.

    ipv6 pim component-id_1-255

Mode | Interface Configuration
Defaults | 1
Example | SEFOS (config-if)# ipv6 pim componentId 1
Notes | This command adds the current VLAN into the specified PIMv6 component.

#### Related Commands

- debug ipv6 pim - Enables or disables PIMv6 globally

- show ipv6 pim component - Displays the component information

### 5.1.17 `ipv6 pim dr-priority`

Sets the designated router priority value configured for the PIMv6 router interface. The `no` form of the command sets the default designated router priority value for the PIMv6 router interface.

    ipv6 pim dr-priority 1-65535

    no ipv6 pim dr-priority

Mode | Interface Configuration
Defaults | 1
Example | SEFOS (config-if)# ipv6 pim dr-priority 100
Notes | The DR sets up multicast route entries and sends corresponding join/prune and register messages on behalf of directly-connected receivers and sources, respectively.

#### Related Commands

- show ipv6 pim interface - Displays the PIMv6 interfaces of the router

### 5.1.18 `ipv6 pim override-interval`

Sets the override interval configured for the PIMv6 router interface. The `no` form of the command sets the default override interval for the PIMv6 router interface.

    ipv6 pim override-interval seconds_0-65535

    no ipv6 pim override-interval

Mode | Interface Configuration
Defaults | 0
Example | SEFOS (config-if)# ipv6 pim override-interval 100
Notes | The override interval is the random amount of time delayed for sending override messages to avoid synchronization of override messages when multiple downstream routers share a multi-access link.

#### Related Commands

- show ipv6 pim interface - Displays the PIMv6 interfaces of the router.

### 5.1.19 `ipv6 pim lan-delay`

Sets the LanDelay configured for the PIMv6 router interface. The `no` form of the command sets the default LanDelay for the PIMv6 router per interface.

    ipv6 pim lan-delay seconds_0-65535

    no ipv6 pim lan-delay

Mode | Interface Configuration
Defaults | 0
Example | SEFOS (config-if)# ipv6 pim lan-delay 120
Notes | The LAN delay inserted by a router in the LAN prune delay option expresses the expected message propagation delay on the interface. It is used by upstream routers to find out the delayed time interval for a Join override message before pruning an interface.

#### Related Commands

- show ipv6 pim interface - Displays the PIMv6 interfaces of the router.

### 5.1.20 `set ipv6 pim lan-prune-delay`

Sets the LanPruneDelay bit configured for the PIMv6 router interface to advertise the LAN delay. The command specifies whether to use LAN prune delay or not.

    set ipv6 pim lan-prune-delay {enable | disable}

Syntax Description | enable - Enables LAN-prune-delay. disable - Disables LAN-prune-delay.
Mode | Interface Configuration
Defaults | Disabled.
Example | SEFOS (config-if)# set ipv6 pim lan-prune-delay enable

#### Related Commands

- show ipv6 pim interface - Displays the PIMv6 interfaces of the router

### 5.1.21 `no ipv6 pim interface`

Deletes the IPv6 PIM Interface. That is, this command destroys the interface at PIMv6.

    no ipv6 pim interface

Mode | Interface Configuration
Example | SEFOS (config-if)# no ipv6 pim interface

#### Related Commands

- show ipv6 pim interface - Displays the PIMv6 interfaces of the router.

### 5.1.22 `debug ipv6 pim`

Enables PIMv6 trace. The `no` form of the command disables PIMv6 trace.

    debug ipv6 pim {[nbr] [grp] [jp] [ast] [bsr] [io] [pmbr] [mrt] [mdh] [mgmt] | [all]}

    no debug ipv6 pim {[nbr] [grp] [jp] [ast] [bsr] [io] [pmbr] [mrt] [mdh] [mgmt] | [all]}

Syntax Description | nbr - Neighbor Discovery traces grp - Group Membership traces jp - Join or Prune traces ast - Assert state traces bsr - Bootstrap/RP traces io - Input Output traces pmbr - Interoperability traces mrt - Multicast Route Table Update traces mdh - Multicast Data Handling traces mgmt - Configuration traces all - All traces
Mode | Privileged EXEC
Example | SEFOS# debug ipv6 pim all
Notes | A 4-byte integer value is specified for enabling the level of debugging. Each bit in the 4-byte integer variable represents a level of debugging. Combinations of levels are also allowed. The user has to enter the corresponding integer value for the bit set.

#### Related Commands

- show ipv6 pim interface - Displays the PIMv6 interfaces of the router.

### 5.1.23 `show ipv6 pim interface`

Displays the PIMv6 interfaces of the router. The command shows the list of interface addresses, the mode of the interface, designated router on that interface, hello interval, join or prune interval of the interface.

    show ipv6 pim interface [{Vlan vlan-id | detail}]

Syntax Description | Vlan - VLAN identifier. detail - Detailed information of the interface.
Mode | Privileged EXEC
Example | SEFOS# show ipv6 pim interface Address IfName/ Ver/ Nbr Qry DR DR IfId Mode Count Interval Address Prio- --------- ----- ----- ------ ------- ------- ----- fe80::2:a00:1 vlan1/33 2/Sparse 0 150 fe80::2:a00:1 1 fe80::2:1400:1 vlan2/34 2/Sparse 0 30 fe80::2:1400:1 1 fe80::2:1e00:1 vlan3/35 2/Sparse 0 30 fe80::2:1e00:1 1
| SEFOS# show ipv6 pim interface vlan 1 Address IfName/ Ver/ Nbr Qry DR DR IfId Mode Count Interval Address Prio- --------- ----- ------ ------ ------- ------ ----- fe80::2:a00:1 vlan1/33 2/Sparse 0 150 fe80::2:a00:1 1
| SEFOS# show ipv6 pim interface detail vlan1 33 is up Internet Address is fe80::2:a00:1 Muticast Switching : Enabled PIM : Enabled PIMv6 : Enabled PIM version : 2, mode: Sparse PIM DR : fe80::2:a00:1 PIM DR Priority : 1 PIM Neighbour Count : 0 PIM Hello/Query Interval : 150 PIM Message Interval : 200 PIM Override Interval : 0 PIM Lan Delay : 0 PIM Lan-Prune-Delay : Disabled PIM Component Id : 1 PIM domain border : disabled

#### Related Commands

- set ipv6 pim - Enables or disables PIMv6

- ipv6 pim query-interval - Sets the frequency at which PIMv6 hello messages are transmitted on the interface

- ipv6 pim message-interval - Sets the frequency at which PIMv6 Join/Prune messages are transmitted on the PIMv6 interface

- ipv6 pim bsr-candidate - Sets the preference value for the local PIMv6 interface as a candidate bootstrap router

- ipv6 pim dr-priority - Sets the designated router priority value configured for the PIMv6 router interface

- ipv6 pim override-interval - Sets the override interval configured for the PIMv6 router interface

- ipv6 pim lan-delay - Sets the LanDelay configured for the PIMv6 router interface

- set ipv6 pim lan-prune-delay - Sets the LanPruneDelay bit configured for the PIMv6 router interface to advertise the lan delay

- no ipv6 pim interface - Deletes an interface at PIMv6 level

- debug ipv6 pim - Enables PIMv6 trace

### 5.1.24 `show ipv6 pim neighbor`

Displays the PIMv6 neighbor(s) information of the router. It displays the neighbor address, the interface used to reach the PIMv6 neighbor, the up time (the time since this neighbor became the neighbor of the local router), expiry time (the minimum time remaining before this PIMv6 neighbor will be aged out), LAN delay and override interval.

    show ipv6 pim neighbor [Vlan vlan-id]

Syntax Description | Vlan - VLAN identifier.
Mode | Privileged EXEC
Example | SEFOS# show ipv6 pim neighbor Nbr If Uptime/ Ver DRPri/ Comp Over- Lan Address Name Expiry Mode Id ride Delay /Idx Interval ------------- --------- ------------ --- ------ ---- ---- ----- fe80::2:a00:a vlan1/33 00:02:33/0 v2 0/S 1 0 0 fe80::2:1400:a vlan2/34 00:02:33/0 v2 0/S 1 0 0 SEFOS# show ipv6 pim neighbor vlan 1 Nbr If Uptime/ Ver DRPri/ Comp Over- Lan Address Name Expiry Mode Id ride Delay /Idx Interval ------------- --------- ------------ --- ------ ---- ---- ----- fe80::2:a00:a vlan1/33 00:02:58/0 v2 0/S 1 0 0

#### Related Commands

- ipv6 pim query-interval - Sets the frequency at which PIMv6 hello messages are transmitted on the interface

- ipv6 pim message-interval - Sets the frequency at which PIMv6 Join/Prune messages are transmitted on the PIMv6 interface

- ipv6 pim bsr-candidate - Sets the preference value for the local PIMv6 interface as a candidate bootstrap router

### 5.1.25 `show ipv6 pim rp-candidate`

Displays the PIMv6 RP-candidate information. It displays the group addresses, the group mask and the RP address that indicates the IP address of the rendezvous point (RP) for the listed PIM Sparse group.

    show ipv6 pim rp-candidate component-id_1-255

Mode | Privileged EXEC
Example | SEFOS# show ipv6 pim rp-candidate 1 CompId GroupAddress/PrefixLength RPAddress/Priority ------ ------------------------- ---------- ------- 1 ff02::e000:0/112 3333::a00:1/192

#### Related Commands

- ipv6 pim rp-candidate rp-address - Sets the address of the interface, which will be advertised as a candidate-RP

- ipv6 pim rp-static rp-address - Sets the address of the interface, which will be advertised as a static-RP

### 5.1.26 `show ipv6 pim rp-set`

Displays the PIMv6 RP-set information. It displays details of the group prefix, RP address, hold time, and expiry time.

    show ipv6 pim rp-set rp-address

Syntax Description | rp-address - Indicates the IPv6 address of the rendezvous point (RP) for the listed PIM sparse group.
Mode | Privileged EXEC
Example | `SEFOS#` show ipv6 pim rp-set 3333::a00:a PIM Group-to-RP mappings ------------------------ Group Address : ff00::Group Mask : 8 RP: 3333::a00:a Component-Id : 1 Hold Time : 102, Expiry Time : 00:00:35

#### Related Commands

- ipv6 pim rp-candidate rp-address - Enables the address of the interface, which will be advertised as a candidate-RP

- ipv6 pim rp-static rp-address - Sets the address of the interface, which will be advertised as a static-RP

### 5.1.27 `show ipv6 pim bsr`

This command displays the PIMv6 BSR information.

    show ipv6 pim bsr component-id_1-255

Mode | Privileged EXEC
Example | SEFOS# show ipv6 pim bsr 1 PIMv2 Bootstrap Configuration For Component 1 ------------------------------------------------ Elected BSR for Component 1 V6 BSR Address : 3333::a00:1 V6 BSR Priority : 100, Hash Mask Length : 126 This System is V6 Candidate BSR for Component 1 V6 BSR Address : 3333::a00:1 V6 BSR Priority : 100

#### Related Commands

- ipv6 pim bsr-candidate - Sets the preference value for the local interface as a candidate bootstrap router

### 5.1.28 `show ipv6 pim rp-static`

Displays the static RP information.

    show ipv6 pim rp-static component-id_1-255

Mode | Privileged EXEC
Example | SEFOS# show ipv6 pim rp-static Static-RP Enabled CompId GroupAddress/PrefixLength RPAddress ------ ------------------------- --------- 1 ff02::1111:2222/64 3333::4444

#### Related Commands

- ipv6 pim rp-static rp-address - Enables or disables the Static RP configuration status

### 5.1.29 `show ipv6 pim component`

Displays the component information.

    show ipv6 pim component component-id_1-255

Mode | Privileged EXEC
Example | SEFOS# show ipv6 pim component 1 PIM Component Information --------------------------- Component-Id: 1 PIM Mode: sparse, PIM Version: 2 Elected BSR: 10.0.0.1 Candidate RP Holdtime: 0

#### Related Commands

- ipv6 pim componentId - Adds the interface to the component

### 5.1.30 `show ipv6 pim thresholds`

Displays threshold configured for SPT, RP thresholds, and rate limit values for both SM and DM.

    show ipv6 pim thresholds

Mode | Privileged EXEC
Example | SEFOS# show ipv6 pim thresholds PIM SPT Threshold Information ----------------------------- Group Threshold : 111 Source Threshold : 222 Switching Period : 100 PIM SPT-RP Threshold Information -------------------------------- Register Threshold : 333 RP Switching Period : 300 Register Stop rate limit : 400

#### Related Commands

- set ip pim threshold - Configures the SPT group or source threshold

- set ip pim spt-switchperiod - Configures the period (in seconds) over which the data rate is to be monitored for switching to shortest path tree

- set ip pim threshold - Sets the threshold at which the RP initiates switching to source specific shortest path tree

- set ip pim rp-switchperiod - Sets the period (in seconds) over which RP monitors register packets for switching to the source specific shortest path tree

- set ip pim regstop-ratelimit-period - Sets the period over which RP monitors number of register packets after sending the register stop message

- set ip pim pmbr - Enables or disables the PMBR status

- ipv6 pim dr-priority - Sets the designated router priority value configured for the router interface

### 5.1.31 `show ipv6 pim mroute`

Displays the IPv6 PIM mroute information.

    show ipv6 pim mroute [ {component-id_1-255 | group  group-address | source source-address} summary]

Syntax Description | component-id_1-255 - Component identifier. group-address - Indicates the PIMv6 multicast group address using the listed RP. source-address - The network address which identifies the sources for which this entry contains multicast routing information. summary - Summary of PIMv6 `mroute` information.
Mode | Privileged EXEC
Example | SEFOS# show ipv6 pim mroute IP Multicast Routing Table -------------------------- Route Flags S: SPT Bit W: Wild Card Bit R: RPT Bit Timers: Uptime/Expires Interface State: Interface, State/Mode PIM Multicast Routing Table For Component 1 (*, ff02::e001:0) ,00:03:54/---3401:510a::3401:51a) Incoming Interface : vlan1 ,RPF nbr : fe80::2:a00:a ,Route Flags : WR Outgoing InterfaceList : vlan2, Forwarding/Sparse ,00:03:54/---
| SEFOS# show ipv6 pim mroute group ff02::e001:0 summary IP Multicast Routing Table -------------------------- Route Flags S: SPT Bit W: Wild Card Bit R: RPT Bit Timers: Uptime/Expires PIM Multicast Routing Table For Component 1 (*, ff02::e001:0) ,00:02:49/---3401:510a::3401:51a) ,Route Flags : WR
| SEFOS# show ipv6 pim mroute source ca8d:5102::ca8d:5102 summary IP Multicast Routing Table -------------------------- Route Flags S: SPT Bit W: Wild Card Bit R: RPT Bit Timers: Uptime/Expires (ca8d:5102::ca8d:5102,ff02::e001:0) ,00:01:04/04:01:45 ,Route Flags : ---
Notes | It shows details of the (S ,G) ,(*,G) and (*,*,RP) entries.

#### Related Commands

- ipv6 pim bsr-candidate - Sets the preference value for the local IPv6 interface as a candidate bootstrap router

Copyright © 2012, Oracle and/or its affiliates. All rights reserved.