Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### STP Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure the Spanning Tree BPDU Receive Status

If the BPDU receive function is disabled, the BPDUs received on that port are ignored.

- Specify the BPDU receive status interface and configure the BPDU receive status.

      SEFOS# configure terminal
      SEFOS(config)# interface extreme-ethernet 0/1

  Valid interfaces include physical interfaces and `port-channel` logical interfaces (`port-channel` port-channel-number).

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |