Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### PVRST+ Administration Guide

Search Scope:

- This Document
- Entire Library

### Default Settings

When the switch comes up, MSTP is enabled. PVRST+ is started and enabled after GVRP is disabled. This table contains the default settings for the RSTP+ software:

Feature | Default Setting
--- | ---
Spanning-tree mode | MSTP
Spanning-tree status | Enabled
Spanning-tree timers | Hello time: 2 secondsForward-delay time: 15 seconds.Maximum-aging time: 20 seconds.
Switch priority | 32768
STP priority (configurable on a per-interface basis) | 128
STP cost (configurable on a per-interface basis) | 2000
PVRST module | Disabled
Port type | Hybrid
GVRP | Enabled
VLAN module | Enabled

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |