Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPFv3 Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure the External Database Limit

This example configures the external database limit in SEFOS1 (router `10.0.0.1`) to 20 entries.

1. Enter Global Configuration mode in SEFOS1.

       SEFOS# configure terminal

2. Enable OSPF globally in the switch SEFOS1.

       SEFOS(config)# ipv6 router ospf

3. Configure the OSPF router ID.

       SEFOS(config-router)# router-id 10.0.0.1

4. Configure the external LSDB limit.

       SEFOS(config-router)# as-external lsdb-limit 20

5. Exit Router Configuration mode.

       SEFOS(config-router)# end

6. View the configuration details.

       SEFOS# show ipv6 ospf

        Router Id: 10.0.0.1            ABR Type:  Standard ABR
        SPF schedule delay: 5 secs     Hold time between two SPFs: 10 secs
        Exit Overflow Interval: 0      Ref BW: 100000         Ext Lsdb Limit: 20
        Trace Value: 0x00000800        As Scope Lsa: 1        Checksum Sum: 0xf4c5
        Demand Circuit: Enable         Passive Interface: Disable
        Nssa Asbr Default Route Translation: Disable
        It is an Area Border Router
        Number of Areas in this router  2
                   Area      0.0.0.0
           Number of interfaces in this area is  1
           Number of Area Scope Lsa: 7      Checksum Sum: 0x30ece
           Number of Indication Lsa: 1      SPF algorithm executed:  22 times
                   Area      0.0.0.6
           Number of interfaces in this area is  1
           Number of Area Scope Lsa: 7      Checksum Sum: 0x4d7f3
           Number of Indication Lsa: 0      SPF algorithm executed:  23 times

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |