Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPFv3 Administration Guide

Search Scope:

- This Document
- Entire Library

### Configuring Neighbors

You can use the neighbor configuration information to create neighbors that allocate memory for the neighbor structure and initialize it with default values. This configuration is also used to activate configured neighbors invoking the NSM with a start or down event. You can configure neighbors only in NBMA networks, but you can then point to multipoint networks.

See IPv6 Example Topology Interface and Host Addresses for the topology used for this configuration.

- Configure an OSPFv3 Neighbor

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |