Skip Navigation Links
Exit Print View
| Oracle Ethernet Switches ### L2 and L3 Deployment Best Practices

Search Scope:

- This Document
- Entire Library

### L2 and L3 Configuration Task Overview

Use these topics to configure the L2 and L3 implementations.

Goal | Links
--- | ---
Learn about the L2 and L3 topology. | L2 and L3 Topology
Learn about the L2 PVRST implementations. | L2 Based Configuration Example Using PVRST Protocol
Configure standard L2 PVRST. | Configuring a Basic L2 PVRST Based Topology
Configure L2 PVRST Active/Standby on the servers. | Configuring an L2 PVRST Based Topology With Active/Standby Bond on the Servers
Configure L2 PVRST LLA Active/Active on the servers. | Configuring an L2 PVRST and LLA Based Topology With Active/Active Bond on the Servers
Learn about the L3 RIP and OSPF implementations. | L3 RIP and OSPF Configuration Overview
Configure L3 RIP. | Configuring L3 Routing Based Topology Using RIP
Configure L3 OSPF. | Configuring L3 Routing Based Topology Using OSPF

##### Related Information

- L2 and L3 Topology

- L2 and L3 VLAN Best Practices

- Adding VLANs

Copyright © 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |