Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPFv3 Administration Guide

Search Scope:

- This Document
- Entire Library

#### Area Route Overview

You can configure ASBR routers in various ways to summarize the routes to different areas. This summary will be advertised, by default. The aggregating routes can be internal address range or AS-external address range. You can configure area parameters only after enabling the OSPF process. Configure these parameters in Router Configuration mode.

Internal address ranges are one of two types:

- Type-3 aggregation

- Type-7 translation aggregation

For AS-external address range aggregation, Type-5 and Type-7 address ranges can be aggregated, and Type-5/Type-7 LSA conversion and generation can also be configured.

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |