Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### DCB Administration Guide

Search Scope:

- This Document
- Entire Library

#### Host Blade Configuration

In a configuration using DCB with SEFOS switches, the host blade (server 1) has the following specifications:

- Sun Dual 10GbE PCIe 2.0 Fabric Expansion Module connected to the switch in slot 0:

  - Linux interface: FEM port 0

  - Switch port number: 18

  - Can also be used to connect to the switch's external ports such as ports 1 or 2.

- Host blade running SUSE 11 2.6.32.12-0.7 or later.

  SEFOS DCB only supports a server with a Sun Dual 10GbE SFP+ PCIe 2.0 ExpressModule Adapter installed.

- Server option: Server running SUSE 11 2.6.32.12-0.7 with Sun Dual 10GbE SFP+ PCIe 2.0 ExpressModule Adapter installed.

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |