Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPFv3 Administration Guide

Search Scope:

- This Document
- Entire Library

### Configuring External Database Limit

Configuring the external database limit provides the upper limit for the number of non-default AS-external-LSAs in a router's link-state database. The router enters overflow state when it reaches the limit. The router does not hold more than the configured non-default AS-external-LSAs in its database.

You must set the LSDB limit identically in all routers that are attached to the OSPFv3 backbone or any regular OSPFv3 area (for example, OSPFv3 stub areas and NSSAs are excluded).

- Configure the External Database Limit

- Restore the Default External Database Limit

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |