Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### PIM Administration Guide

Search Scope:

- This Document
- Entire Library

### Protocol Description

SEFOS PIM is a multicast routing protocol designed to provide scalable inter-domain multicast routing across the internet. PIM provides multicast routing and forwarding capability to a router that runs IP along with IGMP. PIM depends on IGMP for multicast group membership information. PIM routes the multicast data packets independent of any unicast routing protocol. PIM supports two modes of operation: sparse and dense.

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |