Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### MLDS Administration Guide

Search Scope:

- This Document
- Entire Library

### Protocol Description

MLD works with IPv6 to control the reception of multicast data in a network. MLD functions similarly to IGMP, which manages multicast groups for IPv4.

The MLDS function enables switches to forward multicast data to only those hosts that need to receive the data, rather than to all ports. MLDS allows a switch to snoop or capture information from MLD packets that are being sent back and forth between hosts and a router. Based on this information, the switch adds or deletes the multicast addresses from its address table, thereby enabling or disabling multicast traffic that is flowing to individual host ports.

In subnets where MLD is configured, MLDS manages multicast traffic at layer 2.

On a router, MLD periodically sends out MLD queries. When MLD snooping is enabled, the switch responds to the MLD queries with only one MLD join request per multicast group. The switch then creates one entry per subnet in the layer 2 forwarding table for each layer 2 multicast group from which it receives an MLD join request.

A host connected to a layer 2 interface that needs to join an IP multicast group sends an MLD join request specifying the IPv6 multicast group. When a host needs to leave the multicast group, it can either ignore the periodic MLD general queries, or it can send an MLD leave message. If the switch receives an MLD leave message from a host, the switch sends out an MLD group-specific query to determine whether any devices connected to that interface are interested in traffic for the specific multicast group. The switch then updates the table entry for that layer 2 multicast group so that only those hosts that are interested in receiving multicast traffic for the group are listed.

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |