Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### PIM Administration Guide

Search Scope:

- This Document
- Entire Library

### Configuring PMBR Status

A PMBR integrates two different PIM domains (either PIM-SM or PIM-DM) to connect a PIM domain to other multicast-routing domains. You can enable or disable the reporting of PMBR status for a given domain. By enabling PMBR status reporting on a specific router, that router behaves as a PMBR router.

- Enable PMBR Status Reporting

- Disable PMBR Status Reporting

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |