Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### PIMv6 Administration Guide

Search Scope:

- This Document
- Entire Library

## Create a PIMv6 Component

The PIMv6 component corresponds to each instance of a PIMv6 domain. The component is classified as being in the sparse mode. Dense mode is not supported in the 1.2 release.

1. Enable PIMv6.

       SEFOS# configure terminal
       SEFOS(config-if)# set ipv6 pim enable

2. Enter into PIMv6 component mode for configuring a component.

       SEFOS(config)# ip pim component component_ID
       SEFOS(pim-comp)# end

3. Review the configuration information for the component (2 in this example).

       SEFOS# show ipv6 pim component 2

       PIM Component Information
       ---------------------------
       Component-Id: 2
         PIM Mode: sparse,   PIM Version: 2
         Elected BSR: ::
         Candidate RP Holdtime: 0

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |