Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### IGMP Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure the IGMP Robustness Value

1. Enter Interface Configuration mode for `VLAN 2`.

       SEFOS# configure terminal
       SEFOS(config)# interface vlan 2

2. Configure the robustness value as 3.

       SEFOS(config-if)# ip igmp robustness 3
       SEFOS(config-if)# end

3. Ensure that the robustness value has changed.

       SEFOS# show ip igmp interface
       ...
        Robustness value is 3
       ...

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |