Skip Navigation Links
Exit Print View
| Oracle Ethernet Switches ### L2 and L3 Deployment Best Practices

Search Scope:

- This Document
- Entire Library

## Understanding L2 and L3 Implementations

These topics describe L2 and L3 implementations based on a common usage topology with Access and Distribution layer protocols supported by the Oracle Switch ES1-24 (`ES1-24p-n`) and Sun Network 10GbE Switch 72p (`ToR72p-n`).

- L2 and L3 Configuration Task Overview

- L2 and L3 Topology

- L2 and L3 VLAN Best Practices

- Adding VLANs

##### Related Information

- Understanding L2 and L3 Implementations

- L2 Based Configuration Example Using PVRST Protocol

- Configuring a Basic L2 PVRST Based Topology

- Configuring an L2 PVRST Based Topology With Active/Standby Bond on the Servers

- Configuring an L2 PVRST and LLA Based Topology With Active/Active Bond on the Servers

- L3 RIP and OSPF Configuration Overview

- Configuring L3 Routing Based Topology Using RIP

- Configuring L3 Routing Based Topology Using OSPF

Copyright © 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |