Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### MLDS Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure MLDS Query Interval

The MLDS query interval is the period of time the switch waits after sending a group-specific query to determine if hosts are still interested in a specific multicast group. You can configure the group-specific query interval for a given VLAN.

In this example, `VLAN 4` is the VLAN for which the for which the query interval is configured, and the query interval is set to 65 seconds.

1. Configure the MLDS query interval.

       SEFOS# configure terminal
       SEFOS(config)# vlan 4
       SEFOS(config-vlan)# ipv6 mld snooping query-interval 65

2. View the configuration.

       SEFOS# show ipv6 mld snooping

       Snooping VLAN Configuration for the VLAN 4
         MLD Snooping enabled
         MLD Operating version is V1
         Fast leave is disabled
         Snooping switch is configured as Querier
         Snooping switch is acting as Querier
         Query interval is 65 seconds

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |