Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### LA Administration Guide

Search Scope:

- This Document
- Entire Library

### Setting the MTU Value

You can set the MTU value on an individual interface or on the entire port channel. This section contains two example procedures for setting the MTU values.

- Set the MTU Value on one or More Ports

- Set the MTU Value of the Port Channel

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |