Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPFv3 Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure the Host

This example configures SEFOS10 as the host.

1. Enter Global Configuration mode in SEFOS10.

       SEFOS# configure terminal

2. Enable OSPF globally in the switch SEFOS10.

       SEFOS(config)# ipv6 router ospf

3. Configure the OSPF router ID.

       SEFOS(config-router)# router-id 11.0.0.1

4. Configure the host.

       SEFOS(config-router)# host fec0::3556:1:1 metric 10 area-id 0.0.0.1

5. Exit Router Configuration mode.

       SEFOS(config-router)# end

6. View the result of the configuration.

       SEFOS# show ipv6 ospf host

       OSPFV3  HOST  CONFIGURATION Information
       Address                                 AreaId              StubMetric
       fec0::3556:1:1                          0.0.0.1             10

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |