Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPF Administration Guide

Search Scope:

- This Document
- Entire Library

### Configuring the OSPF Testing Authentication Topology Example

The authentication type for OSPF can be configured as Simple Password Authentication, Message-Digest Authentication, or Null Authentication.

Use Interface Configuration mode to perform authentication-related configuration.

Enable OSPF over the VLAN interface and associate the interface with an OSPF area before configuring OSPF authentication. See Enable OSPF Over the VLAN Interface.

- Testing Authentication Topology Example

- Configure Simple Password Authentication

- Configure the Message-Digest Authentication

- Configure the Null Authentication

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |