Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### PIM Administration Guide

Search Scope:

- This Document
- Entire Library

## Specify the Join and Prune Messaging Interval

This example transmits PIM join and prune messages from `VLAN 5` every 120 seconds.

1. Enable PIM globally.

       SEFOS# configure terminal
       SEFOS(config)# set ip pim enable

2. Enter Interface Configuration mode for the interface.

       SEFOS(config)# interface vlan 5

3. Associate the VLAN interface with the PIM component.

       SEFOS(config-if)# ip pim componentId 1

4. Specify how often (in seconds) the switch sends PIM messages to the interface.

       SEFOS(config-if)# ip pim query-interval 60

5. Specify how frequently the PIM interface sends join and prune messages.

       SEFOS(config-if)# ip pim message-interval 120
       SEFOS(config-if)# end

6. Ensure that the correct join and prune messaging interval is set.

       SEFOS# show ip pim interface detail

       Vlan5 33 is up
         Internet Address is 10.1.0.1
         Muticast Switching : Enabled
         PIM : Enabled
         PIMv6 : Disabled
           PIM version : 2, mode: Sparse
           PIM DR : 10.1.0.1
           PIM DR Priority : 1
           PIM Neighbour Count : 0
           PIM Hello/Query Interval : 60
           PIM Message Interval : 120
           PIM Override Interval : 0
           PIM Lan Delay : 0
           PIM Lan-Prune-Delay : Disabled
           PIM Component Id : 1
           PIM domain border : disabled

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |