Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### XVLAN Administration Guide

Search Scope:

- This Document
- Entire Library

### Allowing Regular VLAN on XVLAN Ports

In a normal configuration, ports configured as XVLAN internal and external ports do not allow regular VLAN traffic to be carried. However, in some configurations, it would be desirable to allow both regular VLAN and XVLAN traffic on a given port. Such ports would function as internal or external ports for XVLAN traffic, and would function as they usually would. In addition, these ports function as a trunk port for regular VLANs. To enable this, the regular VLAN must be tagged.

- Configure Regular VLAN on an XVLAN Port

- Display Port VLAN Properties

- Configure Regular VLAN 100 With Ports Used in an XVLAN

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |