Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPFv3 Administration Guide

Search Scope:

- This Document
- Entire Library

### Configuration and Testing Topologies

The examples presented in this guide show various topology scenarios that can be used to configure and test OSPFv3.

The following components are used in the example topology, as shown in IPv6 Example Topology Interface and Host Addresses.

- SEFOS1 through SEFOS9 are SEFOS switches.

- Host A includes host devices that are connected to switch SEFOS3.

- `VLAN 1`, `VLAN 2`, `VLAN 3`, `VLAN 4`, `VLAN 5`, `VLAN 10`, and `VLAN 11` are VLAN interfaces.

- VL represents the virtual link between two areas.

- Each SEFOS switch has a router ID.

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |