Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### STP Administration Guide

Search Scope:

- This Document
- Entire Library

## Restore the Default Transmit Hold Count Value

- Configure the transmit hold count to its default value.

      SEFOS(config)# no spanning-tree transmit hold-count

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |