Skip Navigation Links
Exit Print View
| Sun Network 10GbE Switch 72p ### User’s Guide

Search Scope:

- This Document
- Entire Library

#### Ethernet Cable Cautions

| Caution - Fiber optic Ethernet cables with laser transceivers must be Class I.

| Caution - Do not allow any copper core Ethernet cable to bend tighter than a 5 inch (127 mm) radius. Do not allow any optical Ethernet cable to bend tighter than a 3.4 inch (85 mm) radius. Tight bends can damage the cable internally.

| Caution - Do not use zip ties to bundle or support Ethernet cables. The sharp edges of the ties can damage the cables internally.

| Caution - Do not allow any Ethernet cable to experience extreme tension. Do not pull on an Ethernet cable or allow it to drag. Unroll an Ethernet cable for its length. Pulling on an Ethernet cable can damage the cables internally.

| Caution - Do not twist an Ethernet cable more than 1 revolution for its entire length. Twisting an Ethernet cable can damage the cable internally.

| Caution - Do not route Ethernet cables where they might be stepped upon or experience rolling loads. Such a crushing effect can damage the cable internally.

##### Related Information

- Splitter Cables

- QSFP Cables

- SFP+ Cables

Copyright © 2011, 2012 , Oracle and/or its affiliates. All rights reserved. Legal Notices |