Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPF Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure SEFOS9

1. Configure the area.

       SEFOS# configure terminal
       SEFOS(config)# router ospf

2. Configure ASBR status and redistribute static routes into the OSPF domain.

       SEFOS(config-router)# asbr router
       SEFOS(config-router)# redistribute static
       SEFOS(config-router)# router-id 10.2.2.9
       SEFOS(config-router)# network 10.2.2.9 area 0.0.0.2

3. Configure area `0.0.0.2` as an NSSA area.

       SEFOS(config-router)# area 0.0.0.2 nssa

4. Configure summary address for the range `90.0.0.0/8` in the area `0.0.0.2`.

       SEFOS(config-router)# summary-address 90.0.0.0  255.0.0.0  0.0.0.2
       SEFOS(config-router)# exit

5. Configure static routes.

       SEFOS(config)# ip route 90.1.0.0  255.255.0.0  10.2.2.2
       SEFOS(config)# ip route 90.2.0.0  255.255.0.0  10.2.2.2
       SEFOS(config)# ip route 90.3.0.0  255.255.0.0  10.2.2.2
       SEFOS(config)# ip route 90.4.0.0  255.255.0.0  10.2.2.2
       SEFOS(config)# ip route 90.5.0.0  255.255.0.0  10.2.2.2
       SEFOS(config)# end

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |