Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### PIMv6 Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure the DR Priority Value

Configuring the PIMv6 DR priority configures the designated router priority value for the PIMv6 interface. A designated router sets up multicast route entries and sends corresponding join or prune messages and register messages on behalf of directly connected receivers and sources, respectively.

1. Associate the `VLAN 7` interface with PIMv6 component 1.

       SEFOS(config)# interface vlan 7
       SEFOS(config-if)# ipv6 pim componentId 1
       SEFOS(config-if)# end

2. Set the DR priority to 10.

       SEFOS# configure terminal
       SEFOS(config)# interface vlan 7
       SEFOS(config-if)# ipv6 pim dr-priority 10
       SEFOS(config-if)# end

3. Review the DR priority.

       SEFOS# show ipv6 pim interface detail

       vlan7 34 is up
       ...
           PIM DR Priority: 10
       ...

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |