Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### RIPng Administration Guide

Search Scope:

- This Document
- Entire Library

## Disable Redistribution

The following example disables the redistribution of directly connected routes (`5555::0`) on SEFOS1. With redistribution disabled, the route to `5555::0` is not visible on switches SEFOS2 and SEFOS3.

1. On SEFOS2, review the route information before disabling redistribution.

       SEFOS 2 SEFOS# show ipv6 route

       IPv6 Routing Table  -  6 entries
       Codes : C - Connected, S - Static
               O - OSPF, R - RIP, B - BGP
       C   1111::/112   [1/1]
               via ::, vlan10
       R   2222::/112   [3/120]
               via fe80::221:28ff:fe56:d7a9, vlan40
       R   3333::/112   [2/120]
               via fe80::221:28ff:fe56:d7a9, vlan40
       C   4444::/112   [1/1]
               via ::, vlan40
       R   5555::/112   [2/120]
               via fe80::221:28ff:fe56:d7a9, vlan40
       C   6666::/112   [1/1]
               via ::, vlan10

2. On SEFOS3, review the route information before disabling redistribution.

       SEFOS 3 SEFOS# show ipv6 route
       IPv6 Routing Table  -  7 entries
       Codes : C - Connected, S - Static
               O - OSPF, R - RIP, B - BGP
       R   1111::/112   [3/120]
               via fe80::221:28ff:fe56:d7a9, vlan30
       C   2222::/112   [1/1]
               via ::, vlan20
       C   3333::/112   [1/1]
               via ::, vlan30
       R   3333::/112   [2/120]
               via fe80::221:28ff:fe56:d7a9, vlan30
       R   4444::/112   [2/120]
               via fe80::221:28ff:fe56:d7a9, vlan30
       R   5555::/112   [2/120]
               via fe80::221:28ff:fe56:d7a9, vlan30
       R   6666::/112   [3/120]
               via fe80::221:28ff:fe56:d7a9, vlan30

3. Disable the route redistribution on SEFOS1.

       SEFOS 1 SEFOS# configure terminal
       SEFOS 1 SEFOS(config)# ipv6 route rip
       SEFOS 1 SEFOS(config-router)# no redistribute connected
       SEFOS 1 SEFOS(config-router)# exit

4. On SEFOS2, review the route information after disabling redistribution.

   Note that `5555::/112` [`2/120`] is missing from the output.

       SEFOS 2 SEFOS# show ipv6 route
       IPv6 Routing Table  -  5 entries
       Codes : C - Connected, S - Static
               O - OSPF, R - RIP, B - BGP
       C   1111::/112   [1/1]
               via ::, vlan10
       R   2222::/112   [3/120]
               via fe80::221:28ff:fe56:d7a9, vlan40
       R   3333::/112   [3/120]
               via fe80::221:28ff:fe56:d7a9, vlan40
       C   4444::/112   [1/1]
               via ::, vlan40
       C   6666::/112   [1/1]
               via ::, vlan10

5. On SEFOS3, review the route information after disabling redistribution.

   Note that `5555::/112` [`2/120`] is missing from the output.

       SEFOS 3 SEFOS# show ipv6 route

       IPv6 Routing Table  -  6 entries
       Codes : C - Connected, S - Static
               O - OSPF, R - RIP, B - BGP
       R   1111::/112   [3/120]
               via fe80::221:28ff:fe56:d7a9, vlan30
       C   2222::/112   [1/1]
               via ::, vlan20
       C   3333::/112   [1/1]
               via ::, vlan30
       R   3333::/112   [3/120]
               via fe80::221:28ff:fe56:d7a9, vlan30
       R   4444::/112   [3/120]
               via fe80::221:28ff:fe56:d7a9, vlan30
       R   6666::/112   [3/120]
               via fe80::221:28ff:fe56:d7a9, vlan30

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |