Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### PIMv6 Administration Guide

Search Scope:

- This Document
- Entire Library

### Topology Example

Before enabling PIMv6 in a router, you must configure the router and the host with the IP address and VLAN connectivity. The following example topology is referenced in the configuration steps in this guide.

This topology consists of two routers (router A and router B) with two physical interfaces (`P1` and `P2`), which are `extreme-ethernet 0/1` and `extreme-ethernet 0/2` respectively.

The following table shows the configuration values of the IPv4 and IPv6 addresses for each interface.

Switch or Host | Interface | IPv4 Address | IPv6 Address and Prefix Length
--- | --- | --- | ---
Router A | Port 3 (`VLAN 7`) |  | `7777::11/112`
Port 15 (`VLAN 2`) |  | `2222::12/112`
Port 4 (`VLAN 1`) | `12.0.0.1/24` | `1111::14/112`
Router B | Port 3 (`VLAN 7`) |  | `7777::21/112`
Port 15 (`VLAN 3`) |  | `3333::22/112`
Port 4 (`VLAN 1`) | `12.0.0.2/24` | `1111::24/112`
Host B | Port 3 (`VLAN 3`) |  | `3333::53/112`
Host A | Port 5 (`VLAN 2`) |  | `2222::63/112`

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |