Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### PIM Administration Guide

Search Scope:

- This Document
- Entire Library

### Configuring the PIM Override Interval

The override interval is the random amount of time (in seconds) that override messages are delayed before they are sent to avoid the synchronization of override messages when multiple downstream routers share a multi-access link.

- Specify the Interval to Delay Override Messages

- Restore the Default Override Messaging Interval

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |