Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### IGS Administration Guide

Search Scope:

- This Document
- Entire Library

## Enable the Fast Leave Process

1. Enter the configuration mode for the VLAN interface.

       SEFOS# configure terminal
       SEFOS(config)# vlan 4

2. Enable the fast leave process.

       SEFOS(config-vlan)# ip igmp snooping fast-leave
       SEFOS(config-vlan)# end

3. Review the configuration.

       SEFOS# show ip igmp snooping

       Snooping VLAN Configuration for the VLAN 4
         IGMP Snooping enabled
         IGMP configured version is V3
         Fast leave is enabled
         Snooping switch is configured as Non-Querier
         Snooping switch is acting as Non-Querier
         Query interval is 125 seconds
         Port Purge Interval is 260 seconds
         Max Response Code is 100, Time is 10 seconds

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |