Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### PIMv6 Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure the Rendezvous Point Threshold

Configuring PIMv6 rendezvous point threshold specifies the threshold at which RP initiates switching to the source-specific SPT.

1. Enable PIMv6.

       SEFOS# configure terminal
       SEFOS(config)# set ipv6 enable
       SEFOS(config)# end

2. Set the rendezvous point threshold to 10 seconds.

       SEFOS# configure terminal
       SEFOS(config)# set ip pim rp-threshold 5
       SEFOS(config)# end

3. Review the rendezvous point threshold value.

       SEFOS# show ipv6 pim thresholds

       PIM SPT Threshold Information
       -----------------------------
         Group Threshold  : 0
         Source Threshold : 0
         Switching Period : 0

       PIM SPT-RP Threshold Information
       --------------------------------
         Register Threshold       : 10
         RP Switching Period      : 0
         Register Stop rate limit : 5

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |