Skip Navigation Links
Exit Print View
| Sun Network 10GbE Switch 72p ### User’s Guide

Search Scope:

- This Document
- Entire Library

## Remove an Ethernet Cable

This procedure describes how to remove the cables from the switch chassis, so that a cable can be replaced. If you are removing all cables for switch replacement, start removing the cables from the left side of the switch, working your way to the right.

1. Locate the cable to be removed.
2. Loosen the thumbscrews and remove the cover for the cable management bracket.
3. Grasp the cable connector to support its weight and apply the removal force.
4. Disconnect the cable from the connector.

   - For a dual-part QSFP or SFP+ cable assembly, pull the optical cable connector retraction handle and gently pull out the optical cable.

   - For a single-part passive copper QSFP cable, pull on the retractor strap while simultaneously pulling on the cable connector.

     The cable connector comes free.

5. Carefully move the cable out of the cable management hardware.
6. Gently lower the cable to the floor.

   | Caution - Do not allow the cable to drop or strike the floor. Jerking, bending, pulling on, or dropping the cable can damage the cable.

7. For a dual-part QSFP or SFP+ module assembly, remove the optical transceiver module from the slot.
   1. Pull down the SFP+ or QSFP optical transceiver module latch into the open position.
   2. Slide out the optical transceiver module.
   3. Replace the protective end cap if you plan to store the module.
8. Consider your next step:
   - If you are removing a single cable for replacement, install the new cable.

     See Install an Ethernet Cable.

   - If you are disconnecting all cables for switch replacement, repeat from Step 1 for all cables.

##### Related Information

- Remove a Power Supply

- Remove a Fan

Copyright © 2011, 2012 , Oracle and/or its affiliates. All rights reserved. Legal Notices |