Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### DHCP Administration Guide

Search Scope:

- This Document
- Entire Library

### Two-Switch Configuration

This figure shows the topology for a two-switch configuration. In this example, switch 2 is the DHCP client, except for cases where the Sun Network 10GbE Switch 72p is used.

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |