Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### STP Administration Guide

Search Scope:

- This Document
- Entire Library

### Configuring the Pseudo Root ID

If a port is configured as a layer 2 gateway port, you can use `PseudoRootId` to generate and present the pseudo BPDU to RSTP state machines as if received from another bridge.

Valid interfaces include physical interfaces and `port-channel` logical interfaces (`port-channel` port-channel-number).

- Configure the Pseudo Root ID

- Display the Pseudo Root ID

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |