Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### MLDS Administration Guide

Search Scope:

- This Document
- Entire Library

### Configuring Group Query Interval

When a switch receives a leave message on a port, it sends the group-specific query message on that particular port. You can configure the time interval after which the switch sends a group-specific query on a port. You can also configure the maximum number of group-specific queries sent on a port after an MLD leave message is received.

- Configure the Group Query Interval

- Restore the Default Query Interval

- Configure Group Query Retry Count

- Restore the Default Query Interval

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |