Skip Navigation Links
Exit Print View
| Sun Network 10GbE Switch 72p ### User’s Guide

Search Scope:

- This Document
- Entire Library

#### Motherboard Sensor Targets

Use the targets from this table to check the switch status. See Check Switch Status (Oracle ILOM).

Motherboard Sensor | Target | Comment
--- | --- | ---
CPU temperature | `/SYS/MB/T_CPU` |
I4 temperature | `/SYS/MB/T_SWITCH/`z | where z is 0-8
12V input | `/SYS/MB/V_+12V` |
5V output | `/SYS/MB/V_+5V` |
1.25V for switch chips 1, 2, & 3 | /SYS/MB/V_1V25_SW123 |
1.25V for switch chips 4, 5, & 6 | /SYS/MB/V_1V25_SW456 |
1.25V for switch chips 7, 8, & 9 | /SYS/MB/V_1V25_SW789 |
1.5V output | /SYS/MB/V_1V5 |
2.5V output | /SYS/MB/V_2V5 |
3.3V input | /SYS/MB/V_3V3 |
Battery output | /SYS/MB/V_BAT |
Core voltage | /SYS/MB/V_CORE |
DDR memory | /SYS/MB/V_DDR |

Copyright © 2011, 2012 , Oracle and/or its affiliates. All rights reserved. Legal Notices |