Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPF Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure the ABR Type

This procedure sets the ABR type as either standard, Cisco, or IBM.

1. Enter Global Configuration mode in SEFOS1.

       SEFOS# configure terminal

2. Enable OSPF globally in the switch SEFOS1.

       SEFOS(config)# router ospf

3. Configure the OSPF router ID.

       SEFOS(config-router)# router-id 10.10.2.1

4. Enable OSPF over the VLAN interface and associate the interface with an OSPF area.

       SEFOS(config-router)# network 10.4.0.1 area 0.0.0.0
       SEFOS(config-router)# network 10.10.2.1 area 0.0.0.6

5. Configure the ABR type as Cisco.

       SEFOS(config-router)# abr-type cisco

       The default value ABR type is standard.
       SEFOS# show ip ospf
       OSPF Router ID 10.10.2.1
         Supports only single TOS(TOS0) route
         ABR Type supported is Cisco ABR
         It is an Area Border Router
         Number of Areas in this router is 2
         Area is 0.0.0.6
         Number of interfaces in this area is 1
         SPF algorithm executed 3 times
         Area is 0.0.0.0
         Number of interfaces in this area is 1
         SPF algorithm executed 3 times

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |