Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPFv3 Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure Static Routes

Add static routes to the routing table.

1. Enter Global Configuration mode in SEFOS1.

       SEFOS# configure terminal

2. Add the static route to `3333::/64` through `VLAN 10` with next hop as `fec0::2856:0:1` in SEFOS8.

       SEFOS(config)# ipv6 route 3333:: 64 fec0::2856:0:2

3. Ensure that static routes are properly configured in the SEFOS1 routing table.

       SEFOS# show ipv6 route

       IPv6 Routing Table  -  3 entries
       Codes : C - Connected, S - Static
               O - OSPF, R - RIP, B - BGP
       S   3333::/64   [1/20]
               via fec0::2856:0:2, vlan10
       C   fec0::1111:0:0/96   [1/1]
               via ::, vlan11
       C   fec0::2856:0:0/96   [1/1]
               via ::, vlan10

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |