Skip Navigation Links
Exit Print View
| Sun Network 10GbE Switch 72p ### User’s Guide

Search Scope:

- This Document
- Entire Library

## Glossary

## 10

10GbE

  10 Gigabit Ethernet.

## L

LR

  Long-range. A long-range SFP+ optical tranceiver module.

LR-M

  Long-range multi-mode. A long range multi-mode SFP+ optical tranceiver module.

## O

Oracle ILOM

  Oracle Integrated Lights Out Manager. ILOM provides advanced server processor hardware and software to manage and monitor servers.

## Q

QSFP

  Quad small form-factor, pluggable. A transceiver specification for 4x 10GE modules.

## S

SEFOS

  Sun Ethernet Fabric Operating System. A full-featured fabric and switch management software package for configuring and monitoring the switches network infrastructure.

SEL

  System event log. The switch includes a number of replaceable component sensors that generate entries in the SEL when the sensor crosses a threshold. Many of these readings are used to adjust the fan speeds and perform other actions, such as illuminatiing LEDs and powering off the switch.

SFP+

  Small form-factor, pluggable. A transceiver module specification for several physical layer technologies. In this document, SFP+ refers to Gigabit Ethernet, or 10GbE, modules.

SR

  Short range. A short range SFP+ optical tranceiver module.

switch

  Sun Network 10GbE Switch 72p

## T

TOR

  Top of Rack. The Sun Network 10GbE Switch 72p is a standalone Top of Rack switch.

Copyright © 2011, 2012 , Oracle and/or its affiliates. All rights reserved. Legal Notices |