Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### IGMP Administration Guide

Search Scope:

- This Document
- Entire Library

## Enable the IGMP Proxy Service

You must enable IGMP globally before you enable the IGMP proxy service. You must also disable multicast routing protocols before enabling IGMP proxy service.

1. Enable IGMP.

       SEFOS# configure terminal
       SEFOS(config)# set ip igmp enable

2. Enable the IGMP proxy service in the router.

       SEFOS(config-if)# ip igmp proxy-service
       SEFOS(config-if)# end

3. Review the configuration information.

       SEFOS# show ip igmp global config

       IGMP is globally enabled
       IGMP Proxy is globally enabled in the system

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |